**Cutting Instructions:**

|  |  |
| --- | --- |
| **Mould Base (15x15) Raw** | |
| **Material** | Aluminium |
| **Thickness** | 4mm |
| **Quantity** | 2 |
| **Additional Instructions** | Square hole 150mm x 150mm cut through  2mm 45° chamfer on all four exterior corners |

|  |  |
| --- | --- |
| **Mould Base (20x20)** **Raw** | |
| **Material** | Aluminium |
| **Thickness** | 4mm |
| **Quantity** | 2 |
| **Additional Instructions** | Square hole 200mm x 200mm cut through  2mm 45° chamfer on all four exterior corners |

|  |  |
| --- | --- |
| **Mould Cell Large** | |
| **Material** | Aluminium |
| **Thickness** | 4mm |
| **Quantity** | 400 |

|  |  |
| --- | --- |
| **Mould Cell Small** | |
| **Material** | Aluminium |
| **Thickness** | 2mm |
| **Quantity** | 400 |